**RY-ZH Rotary Dryer**

**Main application and characteristics of the equipment**

Rotary dryer is mainly used for drying fertilizer with certain humidity and particle size, also can be used for drying other materials. The machine has a reasonable design of the distribution and angle of the lifting plate, reliable performance, high utilization of thermal energy, even drying, less cleaning needs of materials, easy to use and maintain.

The simple body part includes spiral material guide area, preheating area, secondary granulation area, combined coping area, granule strengthening and polishing area, and built-in noise reducing vibrator (anti-bonding).

**Main technical parameter**

|  |
| --- |
| Model |
| Drumbody | inner diameter（mm） |
| Length(mm) |
| Rotation speed(r/min) |
| Productivity(T) |
| Motor | Power(kw) |
| Rotation speed(r/min) |
| Reducer Model |

