**RY-GS Tumbler Sieving Machine**

**The main use and characteristics of the equipment**

Tumbler screening machine is a common equipment in the production of organic fertilizer, mainly used for the separation of product and return material, can also achieve the classification of finished products, so the finished products are evenly classified. Adopting combined screen, hoop fixed screen, easy to maintain and replace, the machine has a simple structure, easy to operate, stable operation.

In order to prevent the material from clogging the screen, the tumbler screening machine is equipped with a tapping device.

The technique Parameter

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Model | Cylinder | Rotation speed（r/min） | Inclination (0) | Power(kw) | Productivity(t/h) | Overall Dimension | Weight |
| Diameter (mm) | Length (mm) | Length (mm) x Width (mm) x Height (mm) |
|  |  |  |  |  |  |  |  |  |

